Document Revisions (Title style)

***AISM***Association Internationale de Signalisation Maritime ***IALA***

International Association of Marine Aids to Navigation and Lighthouse Authorities

10, rue des Gaudines

78100 Saint Germain en Laye, France

Telephone: +33 1 34 51 70 01 Fax: +33 1 34 51 82 05

e-mail: [contact@iala-aism.org](mailto:contact@iala-aism.org) Internet: [www.iala-aism.org](http://www.iala-aism.org)

**Draft IALA Guideline No. 1041**

**On**

**Sector Lights**

**Edition 3**

**Intersessional Working Paper ENG 3**

**[2015-10-19]**

**Edition 2: December 2008**

**Edition 1: December 2004**

Revisions to the IALA Document are to be noted in the table prior to the issue of a revised document.

|  |  |  |
| --- | --- | --- |
| **Date** | **Page / Section Revised** | **Requirement for Revision** |
| December 2008 | Whole document | General update |
| ENG 2015 |  | Working paper |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

Table of Contents (Title style)

To update, right click anywhere on the table, then *update field* / *update entire table.*

[Document Revisions (Title style) 1](#_Toc433026607)

[Table of Contents (Title style) 3](#_Toc433026608)

[Index of Tables 5](#_Toc433026609)

[Index of Figures 5](#_Toc433026610)

[Guideline on Sector Lights 7](#_Toc433026611)

[1 introduction 7](#_Toc433026612)

[2 BACKGROUND 7](#_Toc433026613)

[3 Purpose 10](#_Toc433026614)

[4 definitions 10](#_Toc433026615)

[4.1 Sector Light (2-5-215) 10](#_Toc433026616)

[4.2 Angle of uncertainty (2-5-230) 10](#_Toc433026617)

[4.3 Sector Screen / Cut Screen (2-4-125) 10](#_Toc433026618)

[4.4 Vertical Divergence (2-1-200) 10](#_Toc433026619)

[4.5 Total Subtense 10](#_Toc433026620)

[4.6 Sector Accuracy 10](#_Toc433026621)

[4.7 Alternating Sector 10](#_Toc433026622)

[4.8 Oscillating Boundary 11](#_Toc433026623)

[5 Key Parameters of Sector Lights 11](#_Toc433026624)

[5.1 General requirements 11](#_Toc433026625)

[5.2 Angle of uncertainty 12](#_Toc433026626)

[5.3 The Use of filters in sector lights 12](#_Toc433026627)

[6 TYPES OF SECTOR LIGHTS 13](#_Toc433026628)

[7 Point Light Source Sector Lights 14](#_Toc433026629)

[7.1 Single light source and filters 14](#_Toc433026630)

[7.1.1 Principle of operation 14](#_Toc433026631)

[7.1.2 The light source 15](#_Toc433026632)

[7.1.3 Angle of Uncertainty 16](#_Toc433026633)

[7.1.4 Filter size 16](#_Toc433026634)

[7.1.5 Advantages/Disadvantages 18](#_Toc433026635)

[7.2 Multiple Source Sector Light (MSSL) 19](#_Toc433026636)

[7.2.1 Principle of Operation 19](#_Toc433026637)

[7.2.2 Light source 20](#_Toc433026638)

[7.2.3 Angle of Uncertainty 20](#_Toc433026641)

[7.2.4 Advantages 21](#_Toc433026642)

[7.2.5 Disadvantages 22](#_Toc433026643)

[7.3 Single source mutliple tier sector lights 22](#_Toc433026644)

[8 Slot sector light 22](#_Toc433026645)

[8.1 Principle of operation 22](#_Toc433026646)

[8.2 The light source 23](#_Toc433026647)

[8.3 Angle of Uncertainty 24](#_Toc433026648)

[8.4 Advantages/Disadvantages 24](#_Toc433026649)

[8.4.1 Advantages 24](#_Toc433026650)

[8.4.2 Disadvantages 24](#_Toc433026651)

[9 Use of colour filters in rotating optics 24](#_Toc433026652)

[9.1 Principle of Operation 24](#_Toc433026653)

[9.2 The Light Source 25](#_Toc433026654)

[9.3 Angle of Uncertainty 25](#_Toc433026655)

[9.4 Advantages/Disadvantages 25](#_Toc433026656)

[9.4.1 Advantages 25](#_Toc433026657)

[9.4.2 Disadvantages 25](#_Toc433026658)

[10 Rotating Colour Switching Sector Light 25](#_Toc433026659)

[10.1 Principle of operation 25](#_Toc433026660)

[10.2 Light source 27](#_Toc433026661)

[10.3 Angle of uncertainty 27](#_Toc433026662)

[10.4 Advantages 27](#_Toc433026663)

[10.5 Disadvantages 27](#_Toc433026664)

[11 Projector Sector lights 28](#_Toc433026665)

[11.1 Principle of operation 28](#_Toc433026666)

[11.1.1 Single Light Source 28](#_Toc433026667)

[11.1.2 LED Projector Sector lights 29](#_Toc433026668)

[11.2 Angle of uncertainty 29](#_Toc433026669)

[11.3 Advantages/Disadvantage 30](#_Toc433026670)

[11.3.1 Advantages 30](#_Toc433026671)

[11.3.2 Disadvantages 30](#_Toc433026672)

[12 General design methodology 30](#_Toc433026673)

[13 Special design Requirements 33](#_Toc433026674)

[13.1 Sector accuracy 33](#_Toc433026675)

[13.2 Reflections 33](#_Toc433026676)

[13.3 Cleanness of optical path 33](#_Toc433026677)

[14 INSTALLATION AND VERIFICATION 37](#_Toc433026678)

[14.1 Angle definition 37](#_Toc433026679)

[14.2 General remarks 38](#_Toc433026680)

[14.3 Installation of new sector light with factory setup sectors 38](#_Toc433026681)

[14.3.1 Procedure with a datum on the lantern (low accuracy) 38](#_Toc433026682)

[14.3.2 Using a register plate 41](#_Toc433026683)

[14.3.3 The use of simple sight to improve accuracy 44](#_Toc433026684)

[14.3.4 The use of a telescopic sight for maximum accuracy 45](#_Toc433026685)

[14.3.5 Adjustment in workshop or laboratory (factory setup) 47](#_Toc433026686)

[14.4 Installation of a new sector in existing lights 48](#_Toc433026687)

[14.5 Commissioning 49](#_Toc433026688)

[14.6 Effect of weather conditions 51](#_Toc433026689)

[14.7 Use of theodolits for installation, alignment and commissioning 51](#_Toc433026690)

[14.7.1 Introduction 51](#_Toc433026691)

[14.7.2 Preparation before alignment 54](#_Toc433026692)

[14.7.3 Field alignment of sector light 55](#_Toc433026693)

[15 References 60](#_Toc433026694)

Index of Tables

[Table 1 Tungsten filament lamp (colour temperature approx. 3000 K) 12](#_Toc433026695)

[Table 2 Discharge lamp (colour temperature approx. 5500 K) 12](#_Toc433026696)

[Table 3 White LED (colour temperature xKelvin) 13](#_Toc433026697)

[Table 4 Comparison of the difference technologies of sector lights 13](#_Toc433026698)

[Table 5 Compass and reciprocal bearing 37](#_Toc433026699)

Index of Figures

[Figure 1 Several applications for sector lights. 8](#_Toc433026700)

[~~A single sector light marking a narrow channel~~ 9](#_Toc433026701)

[Figure 2 Multiple sectors arrangement marking a channel 9](#_Toc433026702)

[Figure 3 Subtense angle of projected beam 10](#_Toc433026703)

[Figure 4 Alternating sector 11](#_Toc433026704)

[Figure 5 Oscillating boundary 11](#_Toc433026705)

[Figure 6 Alternating flashes for Oscillating boundary 11](#_Toc433026706)

[Figure 7 Angle of uncertainty 12](#_Toc433026707)

[Figure 8 Single light source sector light with drum lens 14](#_Toc433026708)

[Figure 9 Basic operating principle of Point Source Sector Lights 14](#_Toc433026709)

[Figure 10 Internal filters in a light house 15](#_Toc433026710)

[Figure 11 External filters on a small lantern 15](#_Toc433026711)

[Figure 12 Factors that determine the angle of uncertainty in point source type of sector lights 16](#_Toc433026712)

[Figure 13 Observer’s View at the Assumed Nominal Sector Boundary 17](#_Toc433026713)

[Figure 14 Plan View of the Drum Lens 17](#_Toc433026714)

[Figure 15 Filter offset applied on both sector boundaries 18](#_Toc433026715)

[Figure 16 principle of a multiple source sector light 19](#_Toc433026716)

[Figure 17 an omnidirectional sector light with 5 sectors 20](#_Toc433026717)

[Figure 18 Example of a Multiple source LED sector light with four vertical tiers 20](#_Toc433026718)

[Figure 19 Multiple LED sector light with cut screens 21](#_Toc433026719)

[Figure 20 Basic operating principle of Slot Sector Lights 22](#_Toc433026720)

[Figure 21 Light Source Array 23](#_Toc433026721)

[Figure 22 Basic operating principle of Slot Sector Lights (Three light sources and three sectors) 23](#_Toc433026722)

[Figure 23 Rotating Fresnel Lens 25](#_Toc433026723)

[Figure 24 Top view Rotating Colour Switching Sector Light 26](#_Toc433026724)

[Figure 25 Example operation mode for single flashing light of 3 sectors 27](#_Toc433026725)

[Figure 26 Basic operating principle of Projector Sector Lights 28](#_Toc433026726)

[Figure 27 Multiple beam LED projector sector light 29](#_Toc433026727)

[Figure 28 Single beam LED projector sector light with mirrors 29](#_Toc433026728)

[Figure 29 Reduction of the optical white sector 31](#_Toc433026729)

[Figure 30 Re-evaluation of the white sector 32](#_Toc433026730)

[Figure 31 Compass versus reciprocal bearing 38](#_Toc433026731)

[Figure 32 Sector light with datum "North" on top of the lantern and coloured sectors 38](#_Toc433026732)

[Figure 33 Sector light with datum "46°" (TBS) which points to a known landmark 39](#_Toc433026733)

[Figure 34 Levelling a lantern 39](#_Toc433026734)

[Figure 35 Rotating the lantern with a landmark at 226° as the reference point 39](#_Toc433026735)

[Figure 36 Alignment finished 40](#_Toc433026736)

[Figure 37 Commissioning the sector light by a vessel 40](#_Toc433026737)

[Figure 38 Sector Light mounted on a Register Plate 41](#_Toc433026738)

[Figure 39 Example of a Register Plate 42](#_Toc433026739)

[Figure 40 Close-up Sector Light Mounting on a Register Plate 43](#_Toc433026740)

[Figure 41 Graduated Scale marked on the Secondary Mounting Arrangement 43](#_Toc433026741)

[Figure 42 Two different sights 44](#_Toc433026742)

[Figure 43 Sight picture for the two sight examples 44](#_Toc433026743)

[Figure 44 A simple sight mounted on a sector light 45](#_Toc433026744)

[Figure 45 Precision sector light with alignment telescope 45](#_Toc433026745)

[Figure 46 Projector and telescope axis 46](#_Toc433026746)

[Figure 47 View through telescope 46](#_Toc433026747)

[Figure 48 Sample of practical installation with fixed telescope method 46](#_Toc433026748)

[Figure 49 Adjustment to a landmark 47](#_Toc433026749)

[Figure 50 Horizontal alignment in a workshop 47](#_Toc433026750)

[Figure 51 Vertical alignment in a workshop 48](#_Toc433026751)

[Figure 52 Installing new sectors in an existing sector 48](#_Toc433026752)

[Figure 53 Overlapping filters 49](#_Toc433026753)

[Figure 54 Plane filters 49](#_Toc433026754)

[Figure 55 Sector light testing using a boat 50](#_Toc433026755)

[Figure 56 Sector light commissioning 51](#_Toc433026756)

[Figure 57 : Theodolite rotation axis 52](#_Toc433026757)

[Figure 58 Theodolite basic elements 53](#_Toc433026758)

[Figure 59 Simple mechanical theodolit 53](#_Toc433026759)

[Figure 60 Modern theodolite mounted on a tripod 53](#_Toc433026760)

[Figure 61 Assessment of geographic position by portable DGPS 54](#_Toc433026761)

Guideline on Sector Lights

# introduction

Sector lights have been used as an Aid to Navigation (AtoN) since the 19th century. Many different methods are used to provide sector lights. In addition, there are several emerging technologies that may be used to provide sector lights.

# BACKGROUND

A sector light is an aid to navigation that displays different colours and/or rhythms over designated arcs. The colour of the light provides directional information to the mariner.

A sector or a limit between two sectors may indicate a fairway, a turning point, a junction with other channels, a hazard or something else of importance for the navigator.

When a fairway is covered by a white sector, the convention to a vessel approaching the light from the seaward side must be a green sector to starboard and a red sector to port as per IALA Maritime Buoyage System colour convention for Region A; for Region B the colours are reversed. The white sector indicates safe passage, however this does not always hold true in the entire radial length of the sector. The fairway may alternatively be marked with lighted buoys or leading lights.

When designing fairways, consideration should be given to all possible types of aids to navigation to find the best solution for the particular site.

The requirements for sector lights can be a complex task. The process should be carried out with reference to a good quality chart of the area. In many cases, good local knowledge is also required and factors such as tidal flow, currents and background lighting may need to be considered.

A sector light may indicate one or more of the following boundaries of a navigable waterway.

• change of course position;

• shoals, banks, etc;

• an area or position (e.g. an anchorage);

• the deepest part of a waterway;

• position checks for floating aids;

• boundaries of a navigable waterway

Some examples of sector lights applications are illustrated in Figure 1 and Figure 2.




1. Several applications for sector lights.

Light I is a coastal white light with a red sector indicating a danger. In this application high boundary accuracy is not essential.

Light II is a sector light obscured over the shore, with two white sectors indicating a safe channel. The boundary between the red and the green sector also indicates the position of a buoy.

Light III is a sector light with a red light and 4 white sectors indicating four anchorage positions. It is obscured over the shore.

Light IV is a sector light with a white sector indicating a safe channel. It is obscured over the shore.



1. Multiple sectors arrangement marking a channel

Light V in Figure 2 shows two sector lights arranged to create a parallel sector light system. This arrangement has five sectors. Each sector can have its own flash character or colour.

Light VI indicates oscillating boundaries which could be made up of five or seven sectors and can be used to improve identification of the vessels lateral position

# Purpose

The purpose of this document is to provide the IALA membership with guidance on the principles of operation, practical design and installation of sector lights.

This document does not provide guidance on the nautical requirements.

# definitions

Numbers in brackets refer to IALA Dictionary entry.

## Sector Light (2-5-215)

A light presenting different characters (usually different colours) over various parts of the horizon of interest to marine navigation

## Angle of uncertainty (2-5-230)

The horizontal angle of the region of indefinite character near the boundaries of a sector of a sector light.

The limits or boundaries of a sector are not always precisely cut off due to the characteristics of the light source and merging of colours or changing rhythms between adjacent sectors. The transition zone is defined by an "angle of uncertainty".

## Sector Screen / Cut Screen (2-4-125)

An opaque screen so placed as to provide a sharp cut-off to a beam in sector light, and to reduce the angle of uncertainty.

## Vertical Divergence (2-1-200)

Vertical divergence is the total projected angle in the vertical plane. The associated intensity reduction factor must be given with vertical divergence (usually 10%).

## Total Subtense

Total Subtense is the total projected angle in the horizontal plane.



1. Subtense angle of projected beam

## Sector Accuracy

Due to manufacturing tolerances on lenses, filter glasses and lens-mounting systems, the actual location of a sector boundary may be displaced from the intended place. Accuracy is the maximum angle between intended and actual location.

## Alternating Sector

An alternating sector is created by time-slicing of overlapping sector signal, applying a rhythmic character to the white sector and red/green sectors in opposite phase.



1. Alternating sector

## Oscillating Boundary

A method of giving more information of position near the sector boundary to the mariner by creating a light character with alternately flashing colours (Light Vi in Figure 2).



1. Oscillating boundary

On a position on line 1 in Figure 5 the vessel is far outside of the safe channel marked with a fix light. The mariner sees alternating flashes with a long green duration and a short white. Approaching the axis the flash duration of the green flashes will decrease whereas the white flashes increase (Figure 6), so the flash duration of the white flashes become longer than the green ones (line 2). Finally when the save sector is reached, only fixed white light is seen.



1. Alternating flashes for Oscillating boundary

# Key Parameters of Sector Lights

Definitions of the main parameters are presented in section 4. A more detailed description of the relevant concepts are as follows:

* sector width (angular subtense in horizontal plane)
* colour,
* intensity,
* flash character,
* uniformity of intensity across the sector,
* angle of uncertainty between adjacent sectors,
* vertical divergence.

Definitions of main parameters are provided in 4. Detailed description of relevant concepts is provided below.

## General requirements

A sector light should comply with the following specifiations:

* The colour should be in the optimum regions of IALA Recommendation E-200, Part 1 [1].
* The flash characters should conform to IALA Recommendation E-110 [2].
* The calculation of luminous range or intensity should be carried out according to IALA Recommendation E-200, Part 2 [3].
* The measured performance should be in accordance with IALA Recommendation E-200 Part 3 [4]

The current IALA Navguide and specific IALA Guidelines on Light Sources and LED Technology should be considered.

## Angle of uncertainty

The angle of uncertainty is the region where the colour and/or the flash rhythm change. The mariner typically sees a mixture of the two sector characters and this causes an uncertainty where the mariner is unable to distinguish between the two sectors. The understanding of this aspect is very important for the design of a sector light.

In most cases the angle of uncertainty should be as small as possible or defined by the navigational requirement..



1. Angle of uncertainty

The basic mechanisms that determine the achievable minimum angle of uncertainty differ between types of Sector Lights as described below.

## The Use of filters in sector lights

In Sector Lights where optical filtering of a single light source is used, the luminous intensity, and thus the range, of each sector may vary considerably due to different transmission factors of the optical filters.

The spectral characteristic of the light source has a major impact on the light output from a coloured filter. It is necessary to match the light source with a filter material having a suitable spectral transmission, thus providing a light whose chromaticity is within the IALA recommended colour region (see IALA-Recommendation E-200 Part 1 Colours [1]).

The transmission factor of the colour filter will determine the intensity and therefore range of coloured sector. Some typical values of transmission factors are given in the tables below.

1. Tungsten filament lamp (colour temperature approx. 3000 K)

|  |  |
| --- | --- |
| Colour | Transmission |
| Red | 0.08 - 0.25 |
| Green | 0.08 - 0.25 |
| Yellow | 0.50 - 0.70 |

1. Discharge lamp (colour temperature approx. 5500 K)

|  |  |
| --- | --- |
| Colour | Transmission |
| Red | approx. 0.13 |
| Green | approx. 0.22 |
| Yellow | approx. 0.55 |

1. White LED (colour temperature xKelvin)

|  |  |
| --- | --- |
| Colour | Transmission |
| Red | xx |
| Green | xx |
| Yellow | xx |

E.G. a red filter used a discharge lamp will only allow 13% of the light radiated from the white light source.

There are a number of materials, including glass and plastic, suitable for filters. It is generally easier to get large filters in plastic rather than glass. When using plastic filters, the filter material must be ultraviolet stable and be suitably fitted to ensure that the heat generated by the lamps does not distort it.

# TYPES OF SECTOR LIGHTS

There are two basic types of sector lights: omni-directional and directional. Omni-directional sector lights generally cover up to 360 degrees, whereas directional sector lights only cover a relatively small arc.

Many technical solutions exist for generating sectors. They may be categorized in a number of ways, one of which is by the optical method applied. The two most common technologies for the provision of sectored light signals are as follows:

* Point Light Source Sector Lights (for large sector angles or omnidirectional)
  + Single light source and filters
  + Multiple Source Sector Light (MSSL)
* Projector Sector Lights (for small sectors)

Older technologies are:

* Slot sector light
* Use of colour filters in rotating optics

New developments are:

* Rotating colour switching sector light

A comparison between the basic types of Sector Lights is made in table 3.1. A more detailed description of each is shown in Section 4.

1. Comparison of the difference technologies of sector lights

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Type | **Practical**  **Night Time Range** | **Precision/ Angle of uncertainty** | **Max. Sector width** | **Typical Min. Sector width** |
| **Point Source** | Up to 20 M | Medium (0.25º-0.75°) | 360º | 1º |
| **Projected** | Up to 30 M | Very High (1 minute of arc, 0.017º) | 25º | 0.2° |
| **Slot** | Up to 30 M | Low Boundary width is constant with range | 45º | 1º |
| **Rotating colour switching sector light** | Up to 15 M | 1° - 2° | 360° | 8° |
| **Colour filters in rotating optics** | Up to 20 M | 1º - 20° | 360º | 7º |

# Point Light Source Sector Lights

## Single light source and filters

This type of sector light is sometimes referred to as a “traditional sector light” due to the fact that they have been in use with since the 19th century. Another name is 'shadow method sector lights', in which a coloured sector is generated by placing a piece of coloured glass or plastic (such as polycarbonate or acrylic) against the lantern house glazing or against the light itself. This casts a coloured shadow over the water at the required sector.



1. Single light source sector light with drum lens

### Principle of operation

Point source sector lights generally have a single light source, usually a lamp within a drum lens with one or more optical filters placed at some distance, screening the light and producing each sector in the desired colour.




1. Basic operating principle of Point Source Sector Lights


The physical position of the optical filters used with a light source should be mechanically adjustable for proper alignment of the individual sectors and sector boundaries.

In order to ensure sufficiently small angles of uncertainty between sectors, it is important to locate the optical filters at sufficient radial distance from the light source.

The optical filters may be located internally within the lighthouse glazing or external to a lantern.



1. Internal filters in a light house



1. External filters on a small lantern

On small lantern sector lights consisting only of a lantern, the manufacturer may provide fixed internal filters. In the latter case it is not possible to adjust the sector boundary and the angle of uncertainty is likely to be quite large.

### The light source

In a Point Source Sector light, the horizontal dimension of the light source has great influence on the angles of uncertainty (see 7.1.3).

It is important to correctly focus the light source within the optical apparatus as any small mis-alignment can result in altering the sector boundaries. This problem can be overcome by either using a pre-focussed light source or incorporating a means of accurately aligning the light source as each new lamp is installed.

The spectral characteristics of the light source must match the desired spectrum of each coloured sector as mentioned in the section on basic principles. This means that the spectrum of the lights source contains enough red and green.

In general halogen and metal halide lamps achieve good results concerning the aspects above.

### Angle of Uncertainty

The shadow method can be used where very sharp sector boundaries are not required. The angle of uncertainty may be 0.25-0.75° and intensity may vary. As with any optical apparatus, precise positioning of the lamp is essential. The sector boundary will move if the lamp filament is moved, as it might when a lamp is replaced.

In the Point Source type of sector light the ratio between the horizontal dimension of the light source (d) and the distance between the light source and the optical filter (D), determines the angle of uncertainty (db), and thus the width of the boundary region at any given distance from the sector light.



1. Factors that determine the angle of uncertainty in point source type of sector lights

The mathematical relationship between the factors is as follows:

1. db = d/D [radians]
2. Angle of uncertainty = (d/D) x 57 [degrees]

where

d = Horizontal dimension (width) of light source.

D = Distance from filter to light source.

Equation 1 is the angle subtended by the light source width d at the edge of the filter which is distance D away from the light source. The multiplier 57 is an approximate conversion from radians to degrees, 360°/2\*π. In this case, db is the angle between the light source being fully covered by the filter and being completely uncovered by the filter (see Figure 12) when viewed from a distance by an observer.

The angle of uncertainty can be reduced by decreasing the width of the light source or by increasing the radial distance to the coloured filter.

If space on the AtoNs structure is not a limiting factor, it is usually possible to achieve an angle of uncertainty of around 0.5° with this type of sector light.


Equation 1 is known to be somewhat ‘conservative’. Regarding the colour visible from a far distance, it will not change immediately, when the observer enters the sector of uncertainty defined by equation 1.

An exact method for finding the angle of uncertainty based on the observed colour is presented in [9].

### Filter size

When a coloured sector is required, the size of the filter should extend beyond the given sector angle.

The white sector is more intense than the coloured sector which shows a fraction (T) of the intensity of the white sector. As a result the white light will dominate in the transition zone between the two sectors and the resulting colour will be still in the white region (Figure 13).



1. Observer’s View at the Assumed Nominal Sector Boundary

To avoid this, the coloured filter should be made larger by a filter offset. With this measure the intensity of coloured and white light become equal at the sector boundary (Figure 14).



1. Plan View of the Drum Lens

The filter offset distance, the distance between the edge of the filter and the nominal sector boundary, can be determined by the following equation:.



where: *x* is the filter horizontal offset distance in millimetres;

*T* is the filter transmittance as a factor of one;

*d* is the horizontal width (or diameter) of the light source

in millimetres.

The angular offset of the filter (F), the angle between the edge of the filter and the observed sector boundary, can be determined by the following equation:

1. [radians]

or

1.  [degrees]

where: F is the filter horizontal angular offset of the filter edge;

*x* is the filter horizontal offset in millimetres;

*D* is the distance from the centre of the light source to the filter edge

The filter offset occurs at both edges of the filter, so the required angular width of the filter is always greater than the sector angle covered by that filter.

Therefore, for a single sheet of filter material, the width of the sheet should always be greater than the width of the sector by twice the horizontal filter offset (sector width + 2x / sector angle +2 *ϕ*).

Remarks: In practical terms it is often useful to use two pieces of filter material that overlap in the centre of the sector. This allows for some adjustment during the checking procedure.



1. Filter offset applied on both sector boundaries

### Advantages/Disadvantages

Advantages:

* robust design
* retrofitting with new light sources is possible
* relatively small cost
* low maintenance.

Disadvantages:

* possible large angle of uncertainty
* large nominal ranges may not be achievable
* filter degradation

## Multiple Source Sector Light (MSSL)

The principle of a point source sector light can be used with LED as the light source. However the classical point source sector light in most applications requires a light source which radiate light omnidirectional covering 360° of the horizon.

A single LED is restricted to an angular subtense of maximum 180°. Although a single LED can produce an omnidirectional light by the use of a special optic, it is much easier to use multiple LEDs for an omnidirectional LED sector light.

There are additional reasons for the developing MSSL:

* Green and red LEDs have a very saturated colour which fits perfectly into the IALA colour regions. Using optical filter with LED instead is not very efficient. Therefore each sector has its own LED.
* The required small LED components are still limited in luminous intensity. To achieve large ranges / high intensities it is necessary to stack multiple LEDs in a vertical arrangement (tier arrangement).

### Principle of Operation

MSSL produce the sector signals using several LED light sources equipped with individual lenses and beam forming screens that are distributed in horizontal plane as off-centre point sources (Figure 16)..



1. principle of a multiple source sector light

In Figure 17 an arrangement with 5 sectors of the same size but different colours is shown. To increase the total intensity the horizontal arrangement is repeated in for vertical tiers (Figure 18).



1. an omnidirectional sector light with 5 sectors



1. Example of a Multiple source LED sector light with four vertical tiers

### Light source

Although in theory it is possible to build Multiple Source Sector Lights using incandescent light sources and filters, this technology is currently implemented using LED light sources.

Light signal modules employed inside a MSSL may be of varying complexity, ranging from a single unprotected LED/lens assembly to a fully weather proofed LED/lens module with several vertical LED arrays, redundant circuitry and low-level modulation input for control of flashing.

To achieve a small angle of uncertainty it is necessary to use LED with a small luminescent area. Many new high power LEDs (> 50 W) have a large luminescent chip and cannot be used in a MSSL.

### Angle of Uncertainty

Depending on the light source and cut screen geometry implemented for separating the sector signals, usable segment of an MSSL starts at a distance L1 that is typically from tens to a couple of hundreds of meters from the AtoN position (Figure 19). A blind patch of the size of the cut screen (D, typically not exceeding 100 mm) extends to infinity, increasing the sector boundary region slightly.



1. Multiple LED sector light with cut screens

Beginning of the usable segment of an MSSL can be estimated using the following formula:

1. L1 = A x D / d

where

A = Distance from light source to cut screen in [mm];

D = Horizontal extent of the cut screen between sector light sources in [mm];

d = Horizontal dimension of light source in [mm].

Multiple Source Sector Lights are suitable for sites where high precision of sector borders is not required. Angle of uncertainty depends on a particular implementation with typical values in the range of 0.2° to 0.6°, with longer distances from light sources to cut screens (larger enclosure diameters) providing resolution improvements.

Angle of uncertainty should be the input parameter for MSSL design for preliminary estimation of feasibility of MSSL application.

### Advantages

* Once manufactured to site specification, installation on AtoN site requires minimum efforts
* Sectors with widely varying luminous intensities can be implemented inside a single enclosure
* Different sectors can utilise different rhythmic characters
* Sectors with overlapping borders displaying alternating colour signals with isophase rhythmic character at the boundary can be created using a multi-tiered construction
* LED modules with dual (redundant) circuitry can be employed for increased dependability
* Power consumption of optimally combined LED arrays of different sectors is typically lower than in case of single-source-per-tier screened omnidirectional solutions
* Distributed modular design allows to utilize existing lantern house at the AtoN site, bypassing shadowing effect of window frames
* In case of a modular construction, light source replacement can be accomplished efficiently onsite when necessary and does not require re-adjustment of sectors
* Modular design allows stocking of spare modules for extended life cycle support

### Disadvantages

* Once manufactured to site specification, sector configuration cannot be altered
* Not available off-the-shelf - engineering costs are involved in the design process of each sector light

## Single source mutliple tier sector lights



input ?

# Slot sector light

## Principle of operation

Slot sector lights consist of one or more light beams directed to a focal aperture (slot) at some distance. The ratio between the focal aperture width and the distance between the light source (assuming a point source) and the slot aperture defines the horizontal angle of the sector.



1. Basic operating principle of Slot Sector Lights

In the above example, there is only one sector. The principle may however be extended to a number of light sources of different colours yielding a number of sectors of different colours, and if need be different rhythmical characters.



1. Light Source Array



1. Basic operating principle of Slot Sector Lights (Three light sources and three sectors)

Coloured sectors are arranged with coloured glass mounted directly in channels in front of the lamp.

The boundaries are defined with baffle plates. The baffle plates are some millimetres wider than the focal apertures in the lantern house, to compensate for refraction of light around the baffle plate edge and provide the light exactly at the boundary crossing. The baffle plates are mounted in the same way as the filter glass.

Using an array of lamps as the light source, the luminous intensity in different sectors can be altered depending on the number of lamps used in that sector. The lamps can be connected in several separate groups, which are switched on in sequence, thus giving a stable power load and a character like a rotating light. With a Slot Sector Light it is possible to create very distinct boundaries and sectors if the lamps are placed a long distance from the slot.

## The light source

The light source depends on the application. Sealed beam lamps, PAR 56 200W 30V, mounted in simple stands are typically used as a light source. Systems with up to 2 x 96 lamps have been build, but smaller systems also exist with only a couple of boundaries and 3-6 lamps.

An advantage of such a lamp array is that a burned out lamp will not lead to a total loss of light in boundaries or sectors, but only a reduction in luminous intensity in that part of a sector as the boundary is illuminated by several overlapping lamps.

LED technology can be used in the Slot Sector Lights.

## Angle of Uncertainty

The angle of uncertainty is about 1° or more.

## Advantages/Disadvantages

The slot sector light may be used in existing lighthouses but is not recommended for new installation.

### Advantages

* very robust design
* easy to maintain

### Disadvantages

* size of lantern
* low intensities
* low precision

# Use of colour filters in rotating optics

The application of accurate coloured sectors with a classical revolving pencil beam is not easy to achieve. Therefore it is not recommended to use this type of sector lights for new installations.

However, in many situations it is advantageous to use this arrangement to support the existing optic in a lighthouse.

## Principle of Operation

A Rotating Optic Sector Light consists of a central light source inside a circular arrangement of Fresnel lens panels (pencil beam projection). The Fresnel panels rotate around the light source at the rotation centre. The whole optic is surrounded by one or more filters or opaque screens.



1. Rotating Fresnel Lens

## The Light Source

A Classical revolving pencil beam light requires a compact light source to ensure a single flash for each Fresnel lens panel. The colour is produced by filtering (see 5.3).

Preferred light sources are:

* Halogen incandescent lamps
* Metal halide lamps
* Short arc discharge lamps (e.g. xenon lamps)

LED as a light source requires more care.

* In general it is necessary to use an arrangement with more than one LED, so the size of this arrangement should be small enough to produce a single flash for each Fresnel lens.
* Most phosphor converting white LEDs (PCLEDs) have only a small spectral output for Green and Red. As a result the filtered coloured light may be outside the IALA colour regions. Therefore, the white LED and the filter material have to be selected to ensure that the resultant intensity and colour are acceptable.

## Angle of Uncertainty

The angle of uncertainty can be evaluated by the means of the paper 'A Study of Filtered Sector Lights' [9].

## Advantages/Disadvantages

### Advantages

* High intensities available
* Existing optics can be used

### Disadvantages


* low precision, large angle of uncertainty may be several degrees
* susceptible to false flashes
* low colour recognition when flashes are too short

# Rotating Colour Switching Sector Light

## Principle of operation

Rotating LED light sources can be used for producing several light beams of different colours with spatial distribution in sectors as required in particular application. Each combination of an LED and a lens produces a different beam that can be precisely controlled in time during rotation. Each sector signal is produced by the LED/lens system at a specific time when passing through the designated sector. Basic rhythmic character of such light sector system depends on selected speed of rotation.


Figure 27 shows an example with 6 lenses (2 white, 2 green, 2 red). Thus, we obtain an equipment producing 2 white beams, 2 green beams and 2 red beams.



1. Top view Rotating Colour Switching Sector Light

When rotating, an electronic control detects the angular position of the optic and switches on each LED during the passage through the sector required.

For example, when the lens with white LED points into the direction of the white sector, it is programmed to switch on, providing white light only within the limits of the white sector. The same applies for green and red sectors (see Figure 28). In case of blank sectors all LEDs are switched off.



1. Example operation mode for single flashing light of 3 sectors

## Light source

This technology is only possible with fast switching LED.

## Angle of uncertainty

The angle of uncertainty depends on the horizontal divergence of the single beam with typical values of 1° to 4.7°.

## Advantages

* The sector configuration is merely a matter of programming, with the possibility of any kind of configuration, from only one sector of a single color up to complex multiple sectors of different colours.
* The modification of the width of any sectors can be done by programming without the need of physical handling or modification of the equipment.
* High luminous intensities can be achieved in comparison to sector lights which illuminate the whole sector.
* Power consumption is typically lower than in case of single-source-per-tier screened omnidirectional sector light.

## Disadvantages

* Low angular precision
* Mechanical moving parts
* Single point of failure in electronic control
* Only for short flashes

# Projector Sector lights

Projected light is a specialised form of sector light that can generate sharply defined sector boundaries. This feature is particularly useful for applications that require one or more narrow sectors.

## Principle of operation

### Single Light Source

In this type of sector light, an image of the desired sectors is produced, and projected through a lens. While the image of the desired sectors may be produced in a number of ways, the most common way of producing it is by precisely machined optical filters. The principle is the same as in a slide or an overhead projector, focused at infinity. Vertical strips of coloured filter glass, optically ground and highly polished on their edges to fit closely together, are used as the "slide" or "film" to divide the beam into different sectors. The condenser system collects light radiating from the lamp and spreads it uniformly across the coloured filter.

An image of the filter is projected out to infinity. Sector boundaries may appear blurred within the first few hundred metres as they are out of focus, but will be very sharp at working distances.

Small changes in lamp filament position may cause minor changes in intensity within the beam, but will have no effect on the boundary positions, which are fixed by the projection (or objective) lens system.



1. Basic operating principle of Projector Sector Lights

The objective lens and the filter assembly together determine the total subtense. Different objective systems are used to obtain all the different subtenses with optimal efficiency. Generally smaller subtenses require larger objective lenses and longer barrel lengths. A smaller subtense with the same size lamp would provide a greater intensity and range.

A projector Sector Light uses colour to convey information to the mariner about his angular position relative to the light. The process of "colouring" a beam involves filtering out many colours and only allowing the desired colour to pass (see 5.3).

The Sector Light is bright enough to use by day if sufficient power is available to operate the necessary size of lamp.

The size of lamp that can be fitted is limited by physical size constraints of the optical arrangement. If greater ranges are required than can be achieved with the largest lamp then it is possible to operate two projector light units in a bi-form arrangement.


Greater range is achievable by using a smaller subtense for the projector.

### LED Projector Sector lights

LED light sources are available in a range of monochromatic colours and do not need to use coloured filters. They can provide an energy efficient light source for a coloured sector light, as the light is generated directly in the desired colour and no light is wasted by absorption in sector filters. The filter cost is avoided, as are the cleaning problems often associated with filter installations. Because of the spectral characteristics of white LED lights, coloured filters should not be used with these sources.

Using an individual coloured LED projector for every sector, the resultant is a multi beam LED Projector Sector Light (Figure 12). Single beam LED Sector Lights can be created using various methods including the use of mirrors (Figure 13).

This technology requires that the sector limits must be adjusted very carefully relative to each other. ~~It is almost impossible to adjust the sectors on-site.~~



1. Multiple beam LED projector sector light



1. Single beam LED projector sector light with mirrors

## Angle of uncertainty

Some sector projectors can overcome boundary inaccuracies by the design of the projector optics. These projector sector lights are so precise that a complete colour change at a sector boundary occurs over an angle of less than 1 minute (0.02°) in most models. This corresponds to a lateral distance of just 1 metre at a viewing distance of 3.5 km. Nevertheless, precision of certain projectors with high intensity or wider sectors may exceed 6 minutes (0.1°).

In addition the intensity is maintained right to the edge of the beam, and does not reduce the further the observer is away from the axis.

## Advantages/Disadvantage

### Advantages

* High intensities available even for daytime use
* small angle of uncertainty
* compact design
* low power consumption (LED projector)
* power efficient day/night mode switching (LED projector)

### Disadvantages

* supporting structure must be very robust
* difficult to change sector size

# General design methodology

The following procedure shows some steps to find an appropriate design for the required sector light.

Step 1:

Determine the required sectors

The subtense of each sector is given by the nautical requirements.

The design process for a sector light needs to consider the speed and manoeuvrability of vessels likely to be negotiating the sector, how quickly they can respond once they cross a sector boundary and the situations that may develop when other vessels are in the vicinity

For each boundary the angle of uncertainty must be considered depending on the precision of the guidance required.

Step 2

Determine the required luminous range (from nautical requirement), the background illumination and a typical value for the meteorological visibility.

In general the calculation of the luminous intensity is not based on nominal range (Meteorological visibility = 10 nautical miles (M) and no background illumination). Typical values chosen for meteorological visibility in range calculations are 2 to 5 M.

Step 3:

Determine whether a night-only signal is required or a day and night signal.

Step 4:

Determine the required vertical divergence of the luminous intensity distribution. The divergence can be derived from the lowest range the light is used for navigation, the maximum and minimum bridge height, the height of the light and the tidal range (see IALA Guideline No. 1065 on Aids to Navigation Signal Light Beam Vertical Divergence).

Step 5:

Calculate the required intensity for each sector with the tools of IALA Recommendation E-200 on Marine Signal Lights, Part 2 - Calculation, Definition and Notation of Luminous Range.

Step 6:

Determine the flash character for the sector light or each sector, bearing in mind the characters of other nearby AtoN lights.

The flash characters should comply with the nautical requirements. In many cases occulting or isophase characters are preferred to provide ample time for a mariner to recognise the transitional phases that occur at the sector boundary (longer flash length).

For renewable energy systems, the additional energy consumption arising from long flash length must be balanced against the ability of the power system to provide the required energy.

Flash characters are not suitable to use with oscillating boundaries and therefore consideration must be taken of the background lighting for the fixed sectors.

Isophase characters are suitable when using alternating flashing.

After Step 6 the optical parameters for the light are known and in the next steps the optical apparatus is chosen. However in these steps a nautical assessment should still be considered, especially for the angle of uncertainty.

Example 1:

The nominal boundaries of a sector light are 30°, 65°, 105° and 130° (Figure 29). When the angle of uncertainty of the optical apparatus is taken into account, the safe sector should include the angle of uncertainty. This will ensure that the hazardous sector is clearly identified and when the ship is in the angle of uncertainty it will be still in the safe sector.



1. Reduction of the optical white sector

Example 2:

A small channel should be marked by a projector sector light. A first assessment for the safe sector will be derived from the water depth and width of the channel. A re-evaluation will then take into account the width of the vessels, their speed and manoeuvrability, and the angle of uncertainty of the optical apparatus. This will result in a smaller white sector (Figure 30).

To improve visual navigation in this case, additional sectors with alternating flashes (4.7) or oscillating boundaries (4.8Figure 4) should be considered.



1. Re-evaluation of the white sector

Step 7:

Select the type of a sector light from the list in chapter 6.

The preferred types are

* point source sector lights, for large angular subtense and medium accuracy (7),
* projector sector light for small channels, high accuracy and high intensity (8).
* rotating switching sector lights for large angular subtense and high intensity (11).

If the total subtense is large and the sectors need high intensity and accuracy an arrangement of multiple projector and/or point source sector lights should be considered.

Step 8:

If a daytime signal is required:

Check if the daytime range can be achieved with an acceptable effort. Check whether additional AtoNs are needed for daytime (e.g. buoys to mark a single danger or the border of a channel).

The night time reduction of the intensity should be between 1% to 10% of the daytime intensity. However each application should be considered individually by calculating daytime and nighttime luminous range.

The preferred methods for night time reduction are

* pulse with modulation (PWM, LED only) ,
* optical grey filter
* combination of PWM with reduced night mode current (LED only).

Sometimes voltage reduction may be used for lights with incandescent lamps. In this case the colour of the sectors should be checked for low voltage. Whereas the green and red sectors may fulfill the IALA Recommendation on Marine Signal Lights E-200, Part 1 Colurs, it may not be true for the white sector.

Step 9:

Thereafter optical apparatus is selected by considering additional features as:

* power supply,
* mechanical adaption,
* remote monitoring,
* remote control,
* maintenance.

# Special design Requirements

Sector lights are very sensitive to small changes, therefore special requirements are needed for the design of the lantern.

## Sector accuracy

The sector borders may be moved unintentionally from the required position by:

* moving the light source
* moving cut or filter screens
* rotating the lantern or the supporting structure.

Since the bearing of a sector light is critical, structures supporting sector lights must be particularly resistant to twisting to ensure that the sector lights remain accurate.

The light source has to be adjusted exactly in the focal point of the optic even when it is replaced. If a lamp changer is used, it should exactly reproduce the position for each lamp.

The elements which can cause a misalignment should be marked. The maintenance staff should be trained to take care about the precise alignment of the sector boundaries.

## Reflections

Unwanted reflections may be caused by the lantern glazing, the sash bars, obstructions at the light house, etc.

These reflections may produce false flashes, wrong colour or even a wrong sector. Such anomalies can be minimised by tilting the glazing, by using curved panes or by using sector screens. The window glazing should be made of a single plate, Double-glazed windows should not be used because this will increase reflections.

Obstructions of the light path should be avoided and if they are necessary they should be covered with black matt finish.

## Cleanness of optical path

Ice, condensed water or grime on the glazing of a lighthouse or on the optical components of a sector light may cause coloured sectors to appear white. It may also make the light faint or invisible.

The glazing of the lighthouse and the optical components of a sector light should be accessible for cleaning the surfaces. Preparations should be made to avoid ice, condensed water and grime on the lighthouse glazing. This can be done by a small roof above the glazing at the optical path of a sector light or by introducing a window defroster.

**PLEASE HAVE A LOOK HERE!**

**SOME OF THE CONTENT IS NOW IN 12 GENERAL DESIGN METHODOLoGY**

**SOME OF THE CONTENT COULD GO TO DIFFERENT CHAPTERS**

1. Reduced Intensity in White Sector: Yes or No

Intensity in the white sector of incandescent light source can be reduced by 30% using neutral density filter to match the intensities in the coloured sectors. Large differences in luminous intensities of adjacent sectors have negative impact on the boundary resolution.

1. Reflections

Ensure that there are no unwanted reflections from lantern glazing, sash bars, obstructions, etc.

1. Connections to Other Devices

Determine if connection or synchronization is required with other lights, special controllers, monitoring.

1. Vertical divergence regarding short distances

As with all AtoN structures, the design and materials used in the construction of sector lights should be capable of withstanding the forces imposed at the site in storms and be resistant to corrosion, due to the salt laden marine environment. The design of structures should also facilitate maintenance access. The amount of twist and sway of the structure need to be considered in the overall design as excessive movement could undermine the application of the sector light.

Since the bearing of a sector light is critical, structures supporting sector lights must be particularly resistant to twisting to ensure that the sector lights remain accurate.

The sector produced by a sector light should fulfil a number of essential requirements. It should have the right colour, its intensity has to be high enough to provide the required range, the luminous intensity has to fulfil the requirements and it has to cover the correct angle.

* Bearings, directions of leading (range) lines and limits of sectors should always be stated in terms of the bearings that would be seen by the mariner. Bearings may carry a suffix ‘TBS” or True Bearing from Seaward as confirmation.
* The white sector indicates safe passage, however this does not always hold true for the entire length of the sector.
* The boundaries between sectors are always more or less diffuse. This also holds for the boundaries between light and dark sectors.
* Ice or grime on the glazing of a lighthouse may cause coloured sectors to appear white. It may also make the light faint or invisible.
* The lantern glazing (or lantern panes) both absorbs and reflects light. The reflection of a beam against the inside of the glazing may give rise to false flashes of the wrong colour within a sector. Such anomalies can be minimised by tilting the glazing, by using curved panes or by using sector screens.

During the design of Sector Lights, with incandescent special attention should be paid to transmission factors and chromatic characteristics of the optical path. In a sector light having red, white and green sectors, the central white sector is about five times more intense than the colour sectors. It is possible to balance the luminous intensity between sectors using neutral density filters, which reduce the output intensity but does not change the colour, or using intensifying prisms. Where there is no background lighting, it may be appropriate to use a 25% neutral density filter in the white sector to provide the same intensities in all three sectors. With moderate level of background lighting, a 50% neutral density filter can be used instead of clear glass in the white sector. Because most background lighting at night is white, this gives comparable conspicuity within all three sectors.

Reflections in sector lights can be particularly important because of the risk of the reflected light being mistaken for the true sector light by the mariner. When installing sector lights care must be taken to avoid reflections from lantern glazing or obstructions in/ near the sector.

# INSTALLATION AND VERIFICATION

Due to the significant impact of small deviations in alignment of sector lights on navigation safety, it is of importance that engineering, manufacturing and installation are carried out with care.

Proper measurement, installation and verification procedures must be implemented at each stage of the deployment process.

For details on measurement see IALA-Rec. E-200-3.

## Angle definition

Once the sector boundary angles have been determined, these need to be converted from the goniometer scale to a compass bearing and reciprocal compass bearing. This will enable the sectors to be checked with figures published in the List of Lights or with the navigational requirement.

1. Compass and reciprocal bearing

|  |  |  |  |
| --- | --- | --- | --- |
| **Compass Bearing**  **(lighthouse)** | **Reciprocal bearing**  **(ship)** | **Compass Bearing**  **(lighthouse)** | **Reciprocal bearing**  **(ship)** |
| 0 | 180 | 180 | 0 |
| 350 | 170 | 170 | 350 |
| 340 | 160 | 160 | 340 |
| 330 | 150 | 150 | 330 |
| 320 | 140 | 140 | 320 |
| 310 | 130 | 130 | 310 |
| 300 | 120 | 120 | 300 |
| 290 | 110 | 110 | 290 |
| 280 | 100 | 100 | 280 |
| 270 | 90 | 90 | 270 |
| 260 | 80 | 80 | 260 |
| 250 | 70 | 70 | 250 |
| 240 | 60 | 60 | 240 |
| 230 | 50 | 50 | 230 |
| 220 | 40 | 40 | 220 |
| 210 | 30 | 30 | 210 |
| 200 | 20 | 20 | 200 |
| 190 | 10 | 10 | 190 |



1. Compass versus reciprocal bearing

## General remarks

The installation and verification process depends on whether a new piece of equipment is setup or, existing equipment is updated.

Many new sector lights have manufacturer sectors already setup in a laboratory to comply with the customer’s specification. In this case the installation process is reduced to levelling and rotating the lantern into position for correct sector alignment.

On light house wheres existing equipment is being updated with the addition of filter material a more complex process is required. In this case each sector boundary has to be adjusted individually. Some sector lights which are not setup by the manufacturer have to be setup in the same manner.

If replacing an existing light, mark the sector boundaries from the old light on a convenient existing structure. This can be used for confirmation after installation of the replacement light.

## Installation of new sector light with factory setup sectors

### Procedure with a datum on the lantern (low accuracy)

The installation of a new sector light requires that the equipment complies with the particular specification which includes the sectors and a datum. This datum could be a notable local feature (landmark) or North, The sectors should be verified by a test report of the manufacturer.

Figure 32 shows the top of a sector light with a datum showing 'North'.

Figure 33 shows a sector light with a datum for the direction of a given landmark which is at line with 267°



1. Sector light with datum "North" on top of the lantern and coloured sectors



1. Sector light with datum "46°" (TBS) which points to a known landmark

Once the lantern is installed it should be levelled (Figure 34). In many cases this can be done with the help of a spirit level. The lantern should have either a fixed water level or a reference plane which is parallel to the horizontal light fan.



1. Levelling a lantern

Then the lantern is rotated to align with the reference point (Figure 35.), so that the shown sectors of the lantern cover the required sectors of the charts (Figure 36).



1. Rotating the lantern with a landmark at 226° as the reference point



1. Alignment finished

Commissioning of the sector light should be carried out by a vessel. The task is to sail round all sectors and sector boundaries to ensure that the light complies with the navigational requirement. This requires the mariner to carefully observe the change in colour of the light at each sector boundary and recognition of colour change may best be achieved if a fixed light is exhibited for the duration of the commissioning procedure.

Commissioning by a vessel should be carried out at the required range of the lantern and if possible at the lowest range the light can be used.

In Figure 37 an example for commissioning the sectors by a vessel is shown. The sector boundaries are crossed several times to check the right alignment of the sector boundary. While crossing a sector it should be verified that the sector shows the right colour, flash character and intensity.

More details about commissioning can be found in 14.5.



1. Commissioning the sector light by a vessel

### Using a register plate

The adjustment of the sector light may be easier when using a register plate. The register plate shows a drawing of the sectors and the directions to North and the landmark used for the alignment.

The register plate will be mounted permanently underneath the lantern with a gap so that the plate drawing stays visible.



Sector light

Register Plate

1. Sector Light mounted on a Register Plate

The design of the register plate should include slotted fixing holes to enable it to be rotated about its vertical axis so that it can be aligned with the relevant landmarks and/or references. It should also include markings pertinent to the station on which the sector light is to be fitted as follows:

* a true North mark;
* a diametric line at the relative bearing of a previously agreed landmark or landmarks;
* radial lines at the relative bearings of the sector boundaries (optional with TBS);
* colour identification of the sectors
* note: the thickness of the line markings on the register plate should be no more than 0.5mm.



1. Example of a Register Plate

Please note that if the slotted hole for mounting is in line with the landmark bearing line, the nut and bolt may obscure your view along the line (across the plate).

* Place the register plate on the pedestal mounting plate, roughly aligning the true North radial mark on the register plate with true North using a magnetic compass or similar.
* Using nuts and bolts, loosely secure the register plate in its approximate position on the mounting plate (bearing in mind that the plate will have to be turned to finely adjust its position).
* Look along the diametric landmark bearing line marked on the register plate in the direction of its respective landmark and rotate the plate until the diametric line is aligned with the landmark.
* If there are other landmarks, check their respective lines for correct alignment and adjust to get the best compromise between all landmarks.
* Tighten the nuts and bolts carefully and recheck the landmark alignments.
* Mount the sector light assembly above the register plate (see figure x) and loosely secure (bearing in mind that the light will have to be turned to adjust its position).
* Ensure the light is levelled by using the integral level or a spirit level across the top of the light assembly.
* Rotate the light assembly until the true North datum mark on the sector light base (marked during the light range measurement procedure or by the manufacturer) is aligned with the true North radial mark on the register plate.
* If appropriate, ensure all other marks on the lantern perimeter are aligned with their corresponding radial marks on the register plate.
* Tighten the nuts carefully and recheck the alignment with the register plate.

The installation procedure should now be complete but further adjustment or alignment may be necessary during commissioning.




1. Close-up Sector Light Mounting on a Register Plate



1. Graduated Scale marked on the Secondary Mounting Arrangement

### The use of simple sight to improve accuracy

In many cases a datum is not a very precise method for the alignment of a sector light. The accuracy can be improved by using a simple sight. It is composed of front and rear aiming pieces. There are different shapes for the aiming pieces.



1. Two different sights


If a simple sight (alternative: iron sight) is used, the sight picture for the alignment procedure should be explained.

Some sights are called 'open' when the target has to be aligned above the sight pieces. In this case the occlusion of the target is minimized.



1. Sight picture for the two sight examples

The alignment procedure using a simple sight is the same as described in the chapter above (14.3.1).




1. A simple sight mounted on a sector light

### The use of a telescopic sight for maximum accuracy

The accuracy of the alignment on site can be maximised by using an optical or telescopic sight (alignment telescope). It is the preferred method for the installation of precision sector lights with small sector angles (Figure 45).

Some manufacturers use re-locatable filters or screens for the projector. The sectors can be changed in size and position. Some other projectors have fixed sectors, so there is only the need to adjust the projector on the whole.



1. Precision sector light with alignment telescope

The centre of the white sector is often regarded as the optical axis of the projector. In the workshop or light laboratory a telescope with crosshair or reticule is fitted to the projector. The telescope is adjusted so that the centre of the crosshair shows in the direction of the optical axis of the projector. This means that the optical axis of the projector and the telescope are parallel (Figure 46).



1. Projector and telescope axis

During installation, a vessel with high precision positioning equipment should align itself to the centre of the safe sector. The projector is rotated while looking through the telescope, until the vessel appears at the centre of the crosshair.



1. View through telescope



1. Sample of practical installation with fixed telescope method

Remarks:

* It is assumed that the sectors are already correctly set in a laboratory or workshop, so the adjustment with the telescope is the only task during installation. However, it is recommended to check all the sectors by moving across with a ship.
* The adjustment may be done both horizontally and vertically.

Alternative:

In some cases it is more convenient to use a landmark to adjust the projector. The landmark however may not be on the axis of the safe channel but has an angular deviation a to the axis. In this case the telescope has to be adjusted with the angular deviation to the projector axis.



1. Adjustment to a landmark

### Adjustment in workshop or laboratory (factory setup)

For the preliminary adjustment of a projector sector light in a workshop or laboratory the limited viewing or measurement distance has to take be regarded.

The size and location of the sectors can be measured by a goniophotometer or projected on a screen. The projection screen should have a distance of at least 20 m to the projector (Figure 50).

When X is the horizontal distance between the projector axis and the telescope or sight axis, the distance between the screen marks for the axis and the telescope should have a distance X as well. This will ensure that both axes are adjusted parallel to each other.



1. Horizontal alignment in a workshop

The same holds true for the vertical plane. In nearly all cases the telescope is placed a vertical distance Y above the optical axis of the projector. So the mark on the screen must have a distance Y.



1. Vertical alignment in a workshop

## Installation of a new sector in existing lights

A sector can be installed in an existing light by the addition of filter material or opaque screens. At first the nominal size of the filter material and screens should be calculated taking into account the height of the optic, the distance between light source and filter / screen (d) and the sector width (a).



1. Installing new sectors in an existing sector

*S* horizontal length of the filter

*H* vertical height of the filter

1. when *a* in radians
2. when *a* in degree

At the boundaries between a coloured and a white sector, the actual size of the filter material / screen should be greater than the nominal size (see 7.1.4: ).

In practical terms two pieces of filter material that overlap in the centre of the sector should be used if two boundaries need to be adjusted. This allows for some adjustment during the checking procedure (Figure 53).



1. Overlapping filters

The filter material / screen should be installed as far from the light source as possible (normally at the inside of the glazing). It should be moveable during the installation and have a facility to lock it in place once sectors have been commissioned.

If the radius of the filter material is large, the cylindric shape of the filter may be replaced by a set of plane filters (Figure 54).



1. Plane filters

The filters / screens should be installed roughly to the required sector. A theodolite can be used with a datum if practicable.

For the commissioning procedure a ship is required to adjust and verify the correct sectors. It has to be noted that the sector edge may not exactly match up with the filter material / screen edge (see 7.1.4).

## Commissioning

Measurement of sectors should be carried out by at least two experienced observers. Testing should be conducted under good weather and water conditions, preferably clear and transparent air.

Observations made from a long distance should be carried out in complete darkness. Prior to testing, the sector light system should be inspected to ensure that it is functioning correctly and glazing, lens, etc are clean. It is recommended when the light has long eclipses to alter the character to fixed light.

Sector light "angle of uncertainty" is the horizontal angle of the region of indefinite character near the boundaries of a sector of a sector light (e.g. neither white nor red but somewhere in between). Each sector light and even each sector boundary of that light may give a different angle of uncertainty.


For sector boundaries with a wide angle of uncertainty, the bearing at which the change in colour is perceived in one direction may be significantly different to that in the other direction. In this case, each direction should be treated separately and a mean of several recorded bearings for each direction taken. This will result in two mean values, the mean of which can be taken as the sector boundary bearing and the difference of which can be taken as the angle of uncertainty of the sector boundary.

For example, in one direction the change of colour from red to pink may be recorded three times and the mean taken. In the other direction, the change of colour from white to pink may be recorded three times and the mean taken. The mean of these two means would be the sector boundary bearing. The difference between the two means would be the sector boundary angle of uncertainty.


Each mean sector boundary bearing should be compared with the published data for that station and reported accordingly.

It should be borne in mind that on most stand-alone sector lights there is no readily available means of adjusting a sector boundary. Therefore, if there is a significant departure from the published bearing, either the whole beacon has to be turned, which will affect all other sector boundary bearings, or the equipment will have to be returned to shore to be adjusted on a light measuring range. If necessary, the whole light assembly can be rotated to seek an all round compromise between the errors at all sector boundary bearings.

Measurement is carried out at a number of different positions as indicated in Figure 55 presenting one of many methods to ensure that the sectors are correctly marked throughout the usable part of the sectors.



1. Sector light testing using a boat



Boundary for clear white light

Every measurement group contains of about 4 observations

Measurement near to hazard protected by the sector boundary

Determined boundary for white light

Sector of uncertainty

The number of observations varies depending on the length of the border. At least 2 (normally 3-4) locations should be tested, one of which is close and one at the outer end of the sector. The spread of observations is important to determine the angle of uncertainty.

1. Sector light commissioning

However, each uncertainty contribution should be considered carefully for each station and each sector. When using an electronic chart and positioning by DGNSS, the greater the distance between light and vessel, the more accurate the bearing and consequently the lower the angular uncertainty. This increased accuracy is offset by the ability to observe a change of colour in a light when it is much smaller in the eye (smaller subtense angle) and much dimmer. In the case of white/green boundaries, there is potential for colour confusion at low levels of observer illuminance, particularly for flashing lights. At greater distances of observation therefore, the change from white to green, or vice versa, might not be easily distinguishable.

## Effect of weather conditions

Navigators navigating with the help of multi-coloured sector lights are warned about the certain risks prevailing during the cold season. There are always uncertain angles between the sectors, within which it is difficult to determine the colour of the light.

During the cold season the range of these uncertain angles may increase substantially due to snow and ice coating or formation of mist. The light could then be interpreted as white in sectors where it under normal conditions will be seen as coloured. Furthermore a false light in dark sectors, originating from adjacent sectors, might be observed under these same conditions.

When navigating with the help of sector lights it is therefore very important to make sure that the vessel is on the course line by taking frequent and careful positions, especially during the cold season.

## Use of theodolits for installation, alignment and commissioning

### Introduction

A theodolite is a portable precision instrument designed for measure angles in the horizontal and vertical planes. Theodolites are used mainly for surveying applications, e.g. topographic/geographic surveys and surveys for house building, bridge building, road construction etc.


The details of theodolites vary according to their make and type. Older theodolite is typically mechanical build and newer one can be rather complicated with digital display and data memory unit. Modern theodolites or so-called intelligent or ‘total station’ are equipped with integrated electro-optical distance measuring and computerized for saving data into an integrated register.

Basically the theodolite consists of a movable telescope mounted within two perpendicular axes – the horizontal and the vertical axis.


By turning the upper part of the theodolite (around the vertical axis) it is possible to take a bearing on a specific target object and read out the value on a graduated scale. By a clamp devise on the horizontal scale it is possible to set the horizontal scale reading to a desired reading, e.g. when the direction is given from site A to site B. By tilting the telescope (around the horizontal axis) the vertical or the tilt angel can be read out.

The angle of each of these axes can be measured with great precision – typically to second of arc. The scale of theodolite can be graduated in 360° or a 400ᶢ.

It is recommended to select a 360° theodolite for verification and alignment of sector light because it corresponding to the nautical measuring system within degrees (°), minutes (‘) and seconds (“). A 400ᶢ theodolite can be used by a conversion factor but at practical field work it can lead to confusion during the work and errors in the final results.

[](http://www.google.dk/url?sa=i&rct=j&q=&esrc=s&frm=1&source=images&cd=&cad=rja&uact=8&ved=0CAcQjRxqFQoTCKSs2bfBvcgCFYONLAodsUMEGA&url=http://ibis.geog.ubc.ca/courses/geob309/G309_SurveyEx2011W.html&bvm=bv.104819420,d.bGg&psig=AFQjCNGFAWLngqfKAhgr_7MrsVImWNPo2Q&ust=1444759153291525)

1. : Theodolite rotation axis



1. Theodolite basic elements



1. Simple mechanical theodolit

[](http://www.google.dk/url?sa=i&rct=j&q=&esrc=s&frm=1&source=images&cd=&cad=rja&uact=8&ved=0CAcQjRxqFQoTCLm3oYatwMgCFUMOLAod6OYLig&url=http://www.turbosquid.com/3d-models/3d-theodolite-tripod-base-model/723198&bvm=bv.104819420,d.bGg&psig=AFQjCNE24TSmxEeQL_7ueAFjra3bcgXKeQ&ust=1444855852127088)

1. Modern theodolite mounted on a tripod

Commonly the theodolite is mounted on a tripod. The head of the tripod supports the instrument while the feet are spiked to anchor the tripod to ground.

The theodolite is a fragile and expensive instrument and should be handled with care during transport and use. The theodolite is commonly stored away in a shock proof and water tight case equipped with carrying straps. The tripod can be folded together and it is equipped with shoulder straps for easy transport.

### Preparation before alignment

(i) Sectors and geographic position

* Sector and geographic position of the light are published in the List of Lights or with the navigational requirement from the national maritime authority. Boundary angels and bearings of these from sea need to be converted to reciprocal compass bearing when taken bearing with the theodolite from the light (see Table 5).
* If the geographic position of the light is not accurate enough a repositioning must take place before the alignment procedure. The position can be confirmed/ approved by a portable DGPS unit or by a geodetic survey procedure including relevant geographic reference objects.



1. Assessment of geographic position by portable DGPS

(ii) Selection of geographic reference objects

* List and register of geographic reference object are available from national and local geodetic authorities. By studying sea chart and geographic chart and lists, relevant geographic reference objects are selected.
* Details from previously conducted alignments at the same light can provide useful information about previously used reference objects.
* Prefer and select reference object for the baseline in same direction as the sector being aligned.
* Only approved and confirmed reference objects are used for calculation of reference baselines. Bear in mind when selecting reference objects that the geographic object must be clear and observable from the light being aligned.
* Consider obstacles in the sight line and addition to this consider the distance – not to close, but not too far away that it is difficult to see. Commonly lighthouses, church spire, larger building construction etc. are assessed and registered as a geographic reference object.
* In remote area reference objects are typically available in the terrain and marked with a numbered metal plate. In that case the reference object must be marked with a temporary pole with flag to be visible for the operator of the theodolite.
* Select at least 3 geographic reference objects – one for the reference baseline and two for verification of the baseline and position of the light.

(iii) Calculation of reference baselines

* By identified reference objects and the position of the light, it is now possible to calculate baselines/ bearing between the light and the selected reference objects. Commonly national geodetic authority provides a web based service for these calculations. If not it is possible to calculate the bearing direction.

(iv) Pre-test of the alignment procedure

* Due to the complexity of a theodolite it is central to have a trained and experienced observer to operate the instrument and it is recommended to be familiar with the instrument before using it in field.
* Set up the theodolite and think in the baseline and the reference baseline and the sectors being aligned.

### Field alignment of sector light

(i) Weather forecast

* To achieve a good result of the alignment operation it is important to have a good and stable visibility. It is recommended to carry out the operation at nighttime or in daytime in cloudy weather. Avoid sunny days and days with rain and fog/ low visibility due to the difficulty clearly to observe the transition between sectors.
* Local wave height and current must also be considered when using small boat for observation from sea.

(ii) Preparing lantern and coloured filters for aligning sectors

* Pre-installation work must be finished in good time before the alignment procedure.
* The preparation depending on which type the sector light is. Filter sheets in required color and size and addition fittings and stops must be presented.
* Before the alignment procedure taking place filters and lantern with internal sectors must be installed and aligned by taking a coarse bearing over the lantern with the bare eye in direction to reference objects.
* For easy alignment in field calculate the width of the arc of 1°, 45’, 30’ and 15’, and then it is easy to adjust the filter sheet or the lantern during the alignment procedure.

(iii) Setting-up theodolite

* Light and lighthouses vary according geographic place, size of the building and technical equipment. It is not common to have access to place the theodolite exactly over the lantern or optic. At larger lighthouses it is practical and easy to set-up the theodolite at the balcony and at smaller lighthouses it is more practical to set-up the theodolite on ground in front of the lighthouse building.
* Bear in mind that the best result without errors is to set-up the theodolite in same direction/line as the aligning sector.
* Before setting-up and levelling the instrument verify that it is possible to see all selected reference objects and having unobstructed clear view over sea to follow the vessel.

(iv) Alignment procedure

* The theodolite is set-up and the horizontal circle is levelled by bubbles and three foot screws in accordance to the manufactures’ instruction.
* By pointing the telescope to the reference objects chosen as ‘baseline object’ the horizontal graduated scale is set to the bearing calculated from the light to the ‘baseline object’ position.
* After then the telescope is pointed to the additional reference object positions (at least two) and the bearings are read-out on the horizontal scale.
* Readings must be identical to the calculated bearings for each position and is verification of the position of the light.
* It is recommended to have the light in fix light mode during the alignment procedure.
* Communication between vessel and lighthouse is commonly established by VHF radio at a working channel (not channel 16)
* To avoid confusion in the communication it is recommended to agree a plan describing in which order the sectors are aligned.
* Observers location on board the vessel is agreed (e.g. starboard bridge wing) to secure to take a precise bearing to the observer on board.
* The observer must have normal eye vision and normal color vision and addition to this good command and accuracy when reporting observations.
* The vessel is ordered to go to the first sector as agreed (e.g. white/green) and report by VHF which color they observe (example of messages: white, white, white – CUT – green, green, green…)
* To obtain accurate observations the vessel most cross the sector in as narrow as possible angel to the sector. If crossing the sector perpendicularly the crossing will happens very fast and the observer cannot make an accurate observation.
* During the vessels passage through the sector boundary the theodolite is pointing to and following the observer on board the vessel. At the moment the message is ‘cut’ the reading of the theodolite is taken. Depending on the type of sector light the uncertainty can be more and less and this having influence on the reported observation when aligning the sectors.
* The difference between the readings and the final sector is calculated and the result is multiplied by the arc value (mm/°). The color filter sheet or the lantern is moved physical in position according to the result of the calculation.
* After then the procedure is repeated until a satisfied result is obtained. It is recommended to cross the sector boundary at least 3 times from each side – 3 times from white to green and 3 times from green to white, total 6 crossings.
* At traditional point source sector lights every single sector is aligned and the colored sheets are secured by fittings and stops. At modern LED sector light the cutting is factory set and it is only needed to align one of the sector boundaries and then verify the additional sectors.

(v) Final verification of sectors from vessel

* Finally and before leaving the light it is recommended to navigate by vessel in every single boundary shown from the light.
* For verification of safe passage of area with shallow water and rocks echo sounder registrations are appropriated.

(vi) Report


* Finally prepare a report of the alignment and commissioning including following details:
* Name and number of light (List of Lights)
* Date and time (night, day) for the alignment including information of weather condition (visibility, sun, cloudy, rain etc.)
* List of sectors aligned
* Reference objects, position of reference objects and bearing from the aligned light to the used reference objects
* Verification of position of light
* Name of responsible operator of theodolite
* Vessel name and observers name

PICTURES


****




****

****

****





# References

1. IALA Recommendation E-200 on Marine Signal Lights, Part 1 - Colours
2. IALA Recommendation E-110 for the Rhythmic Characters of Lights on Aids to Navigation
3. IALA Recommendation E-200 on Marine Signal Lights, Part 2 - Calculation, Definition and Notation of Luminous Range.
4. IALA Recommendation E-200 on Marine Signal Lights, Part 3 - Measurement
5. IALA NAVGUIDE 2001
6. IALA Guideline 1048 On LED Technologies and their use in Signal Lights.
7. IALA Guideline 1043 on Light Sources used in Visual Aids to Navigation
8. IALA Recommendation E-112 On Leading Lights, Edition 1.1 December 2005
9. IALA Guideline 1023 The Design Of Leading Lines Edition 1.1 December 2005
10. A Study of Filtered Sector Lights by Ian Tutt, March 2012