Document Revisions

This document has been formatted in accordance with the current IALA template

International Association of Marine Aids to Navigation and Lighthouse Authorities

***AISM***Association Internationale de Signalisation Maritime ***IALA***

10, rue des Gaudines

78100 Saint Germain en Laye, France

Telephone: +33 1 34 51 70 01 Fax: +33 1 34 51 82 05

e-mail: [iala-aism@wanadoo.fr](mailto:iala-aism@wanadoo.fr) Internet: [www.iala-aism.org](http://www.iala-aism.org)

**IALA Recommendation**

**O-113**

**On**

**The Marking of Fixed Bridges and Other Structures over Navigable Waters**

**Edition 2**

**June 2011**

**Edition 1 / May 1998**

Revisions to the IALA Document are to be noted in the table prior to the issue of a revised document.

|  |  |  |
| --- | --- | --- |
| **Date** | **Page / Section Revised** | **Requirement for Revision** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

IALA Recommendation on the Marking of Fixed Bridges and Other Structures over Navigable Waters

(Recommendation O-113)

THE COUNCIL:

**RECALLING** the function of IALA with respect to Safety of Navigation, the efficiency of maritime transport and the protection of the environment;

**RECOGNISING** the need to provide guidance on the marking of fixed bridges over navigable waters which is compatible with the IALA Maritime Buoyage System and other Aids to Navigation (MBS);

**RECOGNISING ALSO** that such guidance should enable a common approach to be made world-wide, thus greatly assisting mariners, who, while navigating in waters of different authorities, should not be confused by different marking systems being used on fixed bridges;

**ADOPTS** the recommendation on the marking of fixed bridges and other structures over navigable waters as set out in the annex of this recommendation; and,

**RECOMMENDS** that National Members and other appropriate Authorities providing marine aids to navigation services ensure that the marking of fixed bridges and other structures over navigable waters conforms to the standards and practices specified in the following Sections of this recommendation.

Table of Contents

[Document Revisions 1](#_Toc290047456)

[Table of Contents 4](#_Toc290047457)

[Index of Tables 4](#_Toc290047458)

[Index of Figures 4](#_Toc290047459)

[Annex 5](#_Toc290047460)

[1 GENERAL 5](#_Toc290047461)

[2 SCOPE 5](#_Toc290047462)

[3 BEST POINT(S) OF PASSAGE 5](#_Toc290047463)

[4 BASIC REQUIREMENT( how to mark the navigable channel) 5](#_Toc290047464)

[4.1 VISUAL MARKS 5](#_Toc290047465)

[4.1.1 Colours (for daymarks and lights) 5](#_Toc290047466)

[4.1.2 Marking by day (if considered necessary) 5](#_Toc290047467)

[4.2 Marking by night 6](#_Toc290047468)

[4.3 SOUND SIGNALS 6](#_Toc290047469)

[4.4 RADAR AND RADIO MARKING 7](#_Toc290047470)

[4.4.1 Radar reflectors 7](#_Toc290047471)

[4.4.2 Racons 7](#_Toc290047472)

[4.4.3 AIS AtoN 7](#_Toc290047473)

[5 ADDITIONAL CONSIDERATIONS 7](#_Toc290047474)

[6 Examples of bridge marks 8](#_Toc290047475)

Index of Tables

[Table 1 Title required (Title goes above the table) **Error! Bookmark not defined.**](#_Toc216497068)

Index of Figures

[Figure 1 Single Span (One Way) 8](#_Toc290047476)

[Figure 2 Single Span (Two Way) 9](#_Toc290047477)

[Figure 3 Multi-Span (One Way) 10](#_Toc290047478)

[Figure 4 Multi-Span(Two Way) 11](#_Toc290047479)

Annex

**The Marking of Fixed Bridges over Navigable Waters**

# GENERAL

The following recommendations should be read in conjunction with the IALA MBS. They are intended to supplement the rules of the system where fixed bridges need special marking to ensure their safety and that of vessels navigating beneath them, for example by reason of limited headroom, water depth or the possibility of collision.

Where sea and inland navigation meet, authorities should ensure that the marking of bridges does not conflict with the signs and signals of inland waterways systems.

# SCOPE

This Recommendation should apply to fixed bridges and structures, including floating bridges, overhead pipelines as well as structures under construction that cross navigable waterways or channels.

# BEST POINT(S) OF PASSAGE

In some cases, it may be necessary or desirable to indicate to vessels the most appropriate point(s) to pass under a bridge. These are referred to in this Recommendation as "best point(s) of passage".

These recommendations provide suitable day and night signals for this purpose.

The "best point(s) of passage" will be determined by the competent Authority taking into account all relevant factors, such as:

* maximum available horizontal and vertical clearance
* water depth under the bridge, particularly where it is not uniform
* protection of the bridge piers and other obstructions
* the need to have one way or two way traffic and to indicate that the traffic separation scheme is implemented in a specific span or spans.

# BASIC REQUIREMENT( how to mark the navigable channel)

## VISUAL MARKS

Bridge marking should be in accordance with the direction of buoyage.

### Colours (for daymarks and lights)

In countries in Buoyage Region A

* Green to starboard
* Red to Port.

In countries in Buoyage Region B

* Red to starboard
* Green to Port.

### Marking by day (if considered necessary)

If navigation is possible in the full passage span. the marks should be located on the bridge piers. If navigation is possible only in part of the span, the marks should be located on or under the span, indicating the limits of the navigable channel.

* In countries in Buoyage Region A
* to starboard: a panel showing a solid green equilateral triangle point upwards.
* to port: a panel showing a solid red square.
* In countries in Buoyage Region B
* to starboard: a panel showing a solid red equilateral triangle point upwards.
* to port: a panel showing a solid green square.

The "best point of passage" may be indicated by a circular panel with red and white vertical stripes.

To ensure positive recognition, the Competent. Authority should be satisfied that there is a good contrast between the coloured panels and the colour of the bridge structure. Such a contrast may be achieved by mounting the panels against a white background.

If there is more than one navigable channel under the bridge, the same system should be used for each channel.

Bridge spans other than those marked by red and green lateral marks, e.g. spans to be used by small craft, may be indicated by special yellow marks as prescribed in the IALA MBS.

Consideration should be given to the placement of no entry signage where appropriate.

## Marking by night

Red or green lights may be used to mark the navigable limits of the channel in accordance with the IALA MBS.

If navigation is possible in the full passage span, the lights should be located on the bridge piers. If navigation is possible only in a part of the span, the lights should be located under the span, or on buoy and beacons in the water so placed as to indicate the limits of the navigable channel. Synchronized lights may be used to increase conspicuity.

The "best point of passage" may be indicated by a white light or lights located under the span and exhibiting a safe water mark character.

If there is more than one navigable channel under the bridge, the same system should be used for each channel.

Care should be taken to ensure that all red and green lights have adequate ranges having regard to the circumstances, especially where background lighting makes identification difficult. The lights must be so mounted as to be visible over all relevant areas of the horizon, and not obstructed by parts of the bridge structure.

Bridge spans other than those marked by red and green lateral, e.g. spans to be used by small craft, may be indicated by special yellow lights as prescribed in the IALA MBS.

As an alternative to aid to navigation lights, the daymarks recommended in paragraphs 3.2.1. and 3.2.2. may be floodlit or displayed on an LED panel.

Floodlighting of bridge piers may in some cases give a satisfactory indication of the navigable area and may be considered.

Retroreflecting material of appropriate colour may be used to enhance night time recognition of daymark panels.

## SOUND SIGNALS

One or more sound fog signals may be used to warn the navigator of the presence of a bridge.

Any type of sound fog signal may be used for this purpose.

If a number of sound fog signals are placed at different points on a bridge or its supports, their characters should be different from each other.

## RADAR AND RADIO MARKING

### Radar reflectors

Bridges crossing navigable water are usually clearly recognizable on a radar display. However channel boundaries or bridge piers are seldom clearly distinguishable.

Radar recognition of the bridge piers or channel boundaries may be made possible by radar reflectors located either on dolphins, on buoys or on poles fixed to the bridge structure. Radars on sea going vessels are usually such that the distance between the bridge and the reflectors should be 20 metres or more. To ensure that the reflectors can be clearly distinguished from the bridge structure, practical trials should be carried out.

### Racons

A short range racon may be used to mark the "best point of passage" under a bridge.

Administrations contemplating the use of more than one racon to mark one or more spans must take into account the technical limitations that may exist. Where two racons are used to mark a bridge span the preferred codes should be:

* Starboard: Morse code T(-)
* Port: Morse code B(-···)

Care should be taken to ensure that the racon trace does not unnecessarily obscure echoes from other targets.

### AIS AtoN

AIS AtoN may be used to give information on the "best point(s) of passage" and other information needed to pass under a bridge.

# ADDITIONAL CONSIDERATIONS

1. No entry marks should be considered to inform mariners that a span or one side of the span is forbidden to pass under. This is useful in helping to avoid collisions, striking and groundings.
2. Bridge piers and other obstructions should be marked as determined by the competent Authority.
3. Buoys or beacons may be deployed to enhance the identification of the navigable channel and to mark any restricted areas in accordance with the IALA MBS.

# Examples of bridge marks



Ship Operation (Up Stream)

Single Span (One Way)

1. Single Span (One Way)




Ship Operation (Up Stream)

Single Span (Two Way)

1. Single Span (Two Way)

Multi-Span (One Way)



Up Stream


Up Stream

Up Stream

1. Multi-Span (One Way)

Multi-Span(Two Way)

Up Stream



Up Stream

Up Stream

1. Multi-Span(Two Way)