|  |
| --- |
| IALA Guideline |

XXXX

Producing an e-Navigation operational service description

Edition 1.0

October 2019

Revisions to this IALA Document are to be noted in the table prior to the issue of a revised document.

|  |  |  |
| --- | --- | --- |
| Date | Page / Section Revised | Requirement for Revision |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

1. INTRODUCTION 3

2. SCOPE 3

3. E-navigation service Development process 3

4. Operational Service description 4

5. DEFINITIONS 4

6. ACRONYMS 4

7. REFERENCES 5

List of Figures

Figure 1 Relationship between Maritime Services, Operation Service Description, Technical Services and product specifications. 4

# INTRODUCTION

This guideline is aimed to assist members and/or other international organisations in the development of an Operational Service Description (OSD) for the provision of IMO defined Maritime Services(MS). The Maritime Services are described in an IALA Guideline. An OSD is the interconnection between the high level description of the Maritime Services and the Technical Services to be developed.

## The overarching e-Navigation Architecture

G-1113 e.d. 1 described the overarching e-Navigation Architecture. There the foundation is described regarding the notion of Maritime Service Portfolio’s (MSP), which later evolved to Maritime Services(MS) and it envisaged that it would consist of operational and technical services. Most MS depend on the exchange of data and for that purpose it is essential that a common understanding of the data is described in standardized data models and stored at a central locations. This is wat is done by a S-200 based product specification. There are already a number of product specification available either in the S-200 and S-100 domain. They are a product from a transition from an existing data set to a S-200 product specification with the intend to harmonize and exchange data at an given point in time. This is however not possible for new services such as the envisaged Maritime Services.

As stated in recommendation E-NAV 140 and in G1113 the development of e-Navigation related services should be based on user (information) needs. This means that the objective of the maritime service, the user need, the information need, user requirements, etc is described in a way that it later can be translated in a technical service specification and a technical design by engineers. This is what the purpose is of an Operation Service Description.


# SCOPE

This guideline is intended for business consultant in the maritime domain, information managers, domain architects etc. This guideline is intended to assist them in challenging the providers of the operational services to specify their needs and intended goals so that the can be realised by technical services.

The scope is limited to the production of an OSD.

# E-navigation service Development process

For the development of IT based services an Agile approach is commonly used. In an Agile organization business and IT are working together on the development of the service. They interactively discuss information and user needs etc. and develop the software solution in an iterative way where the usability is frequently demonstrate d to the end user. Information exchange between business and IT is done in a informal setting where teams work together on a daily basis. In the case of the development of e-Navigation Maritime Services this is not possible. Since the information transfer regarding the MS is a pan committee and even pan organization activity. Therefore it is necessary to follow a more top-down way of working where information about an MS is well documented and a defined process is followed. The relation between the different required documents is also leading for the development process. The relation between the documents is represented in figure 1.



1. Relationship between Maritime Services, Operation Service Description, Technical Services and product specifications.

## Requirement traceability

For the development of MS information is transferred between different stakeholders. In the case op information transfer there is a risk that information gets lost. Resulting in loss of functionality at the end of the development process . To mitigate this it is necessary that requirement traceability is a part of the process. IALA G-1133 gives guidance on this topic and should be used for this purpose. Information needs, user needs and requirements should be made explicit and in every step in de the development process it should be made clear how the requirement is fulfilled.

# Operational Service description

The Operational Service Description should provide all the information needed to make a Service Specification and technical design. The operational service description should i.e. describe a full information need analysis and to derived data needs. The operational service should excist of the following main components:

* Context and goal of the operational service
* Relation with MS
* User needs, Information needs, Functional and non-Functional requirements
* Requirements tracibilty matrix

Annex A; The Operational Service Description Template can assist members with the creation of a OSD>

.

# DEFINITIONS

The definition of terms used in this Guideline can be found in the International Dictionary of Marine Aids to Navigation (IALA Dictionary) at <http://www.iala-aism.org/wiki/dictionary>.

# ACRONYMS

# REFERENCES

1. IALA Guideline G-1128
2. IALA Guideline G-1113
3. IALA Guideline G-1133
4. IALA Rec E-NAV 140

1. Template